Re route everything

Move caps away from screw hole

Route rf signal to both poles of dipole

Pick and implement different transistors

Move kill switches back to appropriate position and make them even